**INDEX**

|  |  |  |  |
| --- | --- | --- | --- |
| **PRAC NO.** | **DETAILS** | **DATE** | **SIGN** |
| **1.** | **Configure Routers** |  |  |
| 1.a. | OSPF MD5 authentication |  |  |
| 1.b. | NTP |  |  |
| 1.c. | Syslog server |  |  |
| 1.d. | SSH connections |  |  |
|  |  |  |  |
| **2.** | **Configure AAA Authentication** |  |  |
| 2.a. | Configure a local user account on Router and configure authenticate on the console and vty lines using local AAA. |  |  |
| 2.b. | Verify local AAA authentication from the Router console and the PC-A client. |  |  |
|  |  |  |  |
| **3.** | **Configuring Extended ACLs** |  |  |
| 3.a. | Configure, Apply and Verify an Extended Numbered ACL – Scenario 1 |  |  |
| 3.b. | Configure, Apply and Verify an Extended Numbered ACL – Scenario 2 |  |  |
|  |  |  |  |
| **4.** | **Configure IP ACLs to Mitigate Attacks.** |  |  |
| 4.a | Verify connectivity among devices before firewall configuration. |  |  |
| 4.b. | Use ACLs to ensure remote access to the routers is available only from management station PC-C. |  |  |
| 4.c. | Configure ACLs on to mitigate attacks. |  |  |
|  |  |  |  |
| **5.** | **Configuring IPv6 ACLs** |  |  |
|  |  |  |  |
| **6.** | **Configuring a Zone-Based Policy Firewall** |  |  |
|  |  |  |  |
| **7.** | **Layer 2 Security** |  |  |
| 7.a. | Assign the Central switch as the root bridge. |  |  |
| 7.b. | Secure spanning-tree parameters to prevent STP manipulation attacks. |  |  |
| 7.c. | Enable port security to prevent CAM table overflow attacks. |  |  |
|  |  |  |  |
| **8.** | **Layer 2 VLAN Security** |  |  |
|  |  |  |  |
| **9.** | **Configure and Verify a Site-to-Site IPsec VPN Using CLI** |  |  |
|  |  |  |  |
| **10.** | **Configuring ASA Basic Settings and Firewall Using CLI** |  |  |
| 10.a. | Configure basic ASA settings and interface security levels using CLI |  |  |
| 10.b. | Configure routing, address translation, and inspection policy using CLI |  |  |
| 10.c. | Configure DHCP, AAA, and SSH |  |  |
| 10.d. | Configure a DMZ, Static NAT, and ACLs |  |  |